# Symbol table for METSO AUTOMATION, Device ND9100HT (57E4) - Valve Positioner

variable        characterization_table_index unsigned        16721 
collection      dv1_valve_position        variable        16762 
variable        VOAT_KF_seat_load         float           16500 
command         read_trend_data                           16674 
variable        valve_travel_cntr         float           16506 
command         read_cut_off_type                         16718 
command         read_DAC_direction                        16749 
command         write_load_for_open_low_alimit                 16574 
variable        VDT_KF_deadband           float           16493 
variable        supply_pressure_Units     enumerated      16783 
variable        VOAT_KF_test_sensitivity  float           16498 
variable        VOAT_KF_test_hysteresis   float           16497 
variable        valve_total_travel_wlimit float           16403 
variable        MPST_KF_overshoot         float           16484 
command         write_increase_open                       16518 
variable        trend_data_block_number   unsigned        16657 
variable        histogram_data_0          float           16703 
variable        histogram_data_1          float           16704 
variable        histogram_data_2          float           16705 
variable        histogram_data_3          float           16706 
variable        histogram_data_4          float           16707 
variable        histogram_data_5          float           16708 
variable        histogram_data_6          float           16709 
variable        histogram_data_7          float           16710 
variable        histogram_data_8          float           16711 
variable        histogram_data_9          float           16712 
command         write_valve_reversals_wlimit                 16557 
variable        actuator_package_info     unsigned        16539 
variable        cylinder_pressure_C2_Units enumerated      16779 
variable        valve_test_control        enumerated      16619 
command         read_valve_package_info                   16550 
command         write_stiction_latch_number                 16573 
method          cancel_test                               16753 
variable        travel_rate_dec           float           16395 
variable        VOAT_KF_SR_C2O_close      float           16503 
menu            VOAT_key_figures_menu                     16477 
variable        setpoint_low_limit        float           16392 
menu            valve_configuration_menu                  16438 
variable        VDT_time_between_steps    float           16610 
command         init_multipoint_step_test                 16603 
command         write_setpoint_cut_off_high                 16524 
command         write_steady_state_dev_latch_time                 16570 
variable        MPST_KF_starting_point    float           16479 
variable        valve_setpoint_Value      float           16792 
method          travel_calib_and_tuning_method                 16452 
variable        VDT_init_time             float           16611 
menu            DLT_key_figures_menu                      16476 
variable        stiction_low_alimit       float           16423 
variable        VDT_KF_testing_time       float           16492 
command         write_valve_total_travel_wlimit                 16556 
command         read_VOAT_key_figures                     16625 
collection      dv2_cylinder_pressure_c1  variable        16763 
method          start_voat_method                         16473 
variable        valve_position_Units      enumerated      16775 
unit            position_units_relation                   16757 
command         read_positioner_fail_action                 16719 
variable        event_class               unsigned        16677 
variable        valve_package_info        unsigned        16549 
command         write_load_for_open_high_wlimit                 16567 
variable        supply_pressure_latch_time float           16417 
variable        DLT_KF_input_signal       float           16490 
command         write_spool_total_travel_wlimit                 16560 
method          read_events_method                        16458 
variable        total_operation_time_cntr float           16505 
variable        DAC_direction             enumerated      16429 
command         read_valve_type                           16533 
variable        spool_valve_travel_cntr   float           16512 
variable        signal_dir                enumerated      16391 
command         read_MPST_key_figures                     16622 
command         init_valve_deadband_test                  16612 
menu            valve_tests_menu                          16433 
unit            control_value_units_relation                 16758 
method          travel_calibration_method                 16450 
variable        number_of_points          unsigned        16620 
collection      dv3_cylinder_pressure_c2  variable        16764 
variable        actuator_reversals_cntr   float           16509 
command         write_stiction_high_alimit                 16572 
command         read_HART_board_sno                       16586 
variable        supply_pressure_low_alimit float           16415 
method          check_cut_offs_method                     16521 
variable        charac_table_data_1       float           16722 
variable        charac_table_data_2       float           16723 
variable        charac_table_data_3       float           16724 
variable        charac_table_data_4       float           16725 
variable        charac_table_data_5       float           16726 
variable        performance_level         enumerated      16389 
collection      dv6_temperature           variable        16767 
variable        charac_table_data_6       float           16727 
variable        charac_table_data_7       float           16728 
variable        charac_table_data_8       float           16729 
variable        charac_table_data_9       float           16730 
command         write_stiction_low_alimit                 16571 
variable        valve_setpoint_Units      enumerated      16793 
variable        loop_current_Value        float           16788 
method          set_quick_1_50_curve_method                 16448 
variable        event_time_1              float           16678 
variable        event_time_2              float           16679 
variable        cylinder_pressure_C2_Value float           16778 
variable        event_time_3              float           16680 
variable        event_time_4              float           16681 
variable        event_time_5              float           16682 
variable        event_time_6              float           16683 
variable        event_time_7              float           16684 
variable        event_time_8              float           16685 
variable        event_time_9              float           16686 
command         write_dynamic_state_dev_wlimit                 16563 
variable        device_test_status        enumerated      16588 
variable        VC_board_sno              ascii           16465 
command         write_DAC_direction                       16750 
command         write_load_for_open_latch_number                 16576 
variable        MPST_KF_td                float           16482 
variable        setpoint_reversals_cntr   float           16511 
variable        valve_dead_angle          float           16388 
command         write_dev_temperature_high_alimit                 16581 
menu            device_lock_menu                          16437 
variable        device_sno                ascii           16467 
variable        VOAT_KF_SR_O2C_open       float           16502 
command         select_flow_characterization_type                 16519 
variable        load_for_open_high_alimit float           16427 
variable        load_for_open_low_wlimit  float           16413 
variable        temperature_Units         enumerated      16785 
menu            diagnostics_menu                          16434 
variable        VOAT_KF_starting_point    float           16494 
variable        event_index               unsigned        16675 
variable        DLT_KF_max_error          float           16489 
variable        VDT_KF_starting_point     float           16491 
command         read_diagnostics_warning_limits                 16568 
variable        histogram_data_item_selector unsigned        16702 
command         read_bypass_signal_modifications                 16544 
command         write_spool_reversals_wlimit                 16561 
variable        actuator_type             enumerated      16385 
variable        cut_off_type              enumerated      16716 
menu            main_menu                                 16430 
command         write_actuator_reversals_wlimit                 16559 
variable        test_data_20              unsigned        16651 
variable        test_data_21              unsigned        16652 
variable        test_data_22              unsigned        16653 
variable        test_data_23              unsigned        16654 
variable        test_data_24              unsigned        16655 
variable        cut_off_high              float           16397 
variable        event_number_10           enumerated      16697 
variable        DLT_init_time             float           16607 
variable        stiction_low_wlimit       float           16411 
command         read_DAC_board_revisions                  16595 
variable        test_data_10              unsigned        16641 
variable        test_data_11              unsigned        16642 
variable        test_data_12              unsigned        16643 
variable        DLT_ending_point          float           16605 
variable        test_data_13              unsigned        16644 
variable        test_data_14              unsigned        16645 
variable        test_data_15              unsigned        16646 
variable        diag_reset_select         enumerated      16591 
variable        test_data_16              unsigned        16647 
variable        test_data_17              unsigned        16648 
variable        test_data_18              unsigned        16649 
command         read_VDT_key_figures                      16624 
variable        test_data_19              unsigned        16650 
menu            VDT_key_figures_menu                      16478 
command         write_load_for_open_low_wlimit                 16566 
menu            MPST_key_figures_menu                     16475 
command         write_dev_temperature_low_alimit                 16580 
command         read_test_data                            16656 
variable        process_application_info  unsigned        16552 
unit            control_value_units_relation_2                 16759 
command         write_device_sno                          16594 
menu            start_tests_menu                          16453 
command         write_dev_temperature_latch_time                 16582 
variable        test_data_0               unsigned        16631 
collection      dv9_HART_error_rate       variable        16770 
variable        test_data_1               unsigned        16632 
variable        test_data_2               unsigned        16633 
variable        test_data_3               unsigned        16634 
variable        test_data_4               unsigned        16635 
command         write_steady_state_dev_alimit                 16569 
variable        HART_error_rate_Units     enumerated      16791 
variable        test_data_5               unsigned        16636 
variable        test_data_6               unsigned        16637 
variable        stiction_latch_number     float           16425 
variable        test_data_7               unsigned        16638 
variable        VOAT_KF_stable_time       float           16495 
variable        test_data_8               unsigned        16639 
command         write_process_application_info                 16554 
variable        test_data_9               unsigned        16640 
variable        loop_current_Units        enumerated      16789 
collection      dv4_pressure_difference   variable        16765 
command         read_event_log                            16700 
variable        MPST_ending_point         float           16600 
command         write_HART_board_sno                      16587 
menu            custom_table_menu                         16441 
variable        charac_table_data_10      float           16731 
variable        charac_table_data_11      float           16732 
variable        charac_table_data_12      float           16733 
variable        MPST_KF_t86               float           16483 
variable        charac_table_data_13      float           16734 
variable        charac_table_data_14      float           16735 
variable        stiction_high_wlimit      float           16412 
variable        charac_table_data_15      float           16736 
variable        DAC_board_HW_rev          ascii           16468 
variable        charac_table_data_16      float           16737 
variable        charac_table_data_17      float           16738 
command         read_valve_dead_angle                     16542 
variable        charac_table_data_18      float           16739 
variable        charac_table_data_19      float           16740 
variable        setpoint_high_limit       float           16393 
variable        charac_table_data_20      float           16741 
variable        pressure_difference_Units enumerated      16781 
variable        charac_table_data_21      float           16742 
unit            position_units2_relation                  16760 
variable        charac_table_data_22      float           16743 
method          set_quick_1_25_curve_method                 16444 
variable        calib_command             unsigned        16529 
method          reset_counters_method                     16514 
command         write_VC_board_sno                        16585 
variable        load_for_open_low_alimit  float           16426 
command         write_actuator_total_travel_wlimit                 16558 
variable        dev_temperature_high_alimit float           16419 
variable        VOAT_KF_load_for_opening  float           16499 
command         write_positioner_fail_action                 16720 
command         init_valve_offline_analysis_test                 16617 
variable        actuator_reversals_wlimit unsigned        16406 
variable        dynamic_state_dev_wlimit  float           16410 
variable        split_range_low           float           16398 
variable        cylinder_pressure_C1_Units enumerated      16777 
variable        stiction_high_alimit      float           16424 
menu            characterization_menu                     16440 
unit            temperature_units_relation                 16756 
method          start_dlt_method                          16472 
command         write_use_limits                          16548 
item-array      characterization_table    variable        16744 
variable        actuator_total_travel_wlimit float           16405 
collection      dv7_spool_position        variable        16768 
command         write_steady_state_dev_wlimit                 16562 
variable        steady_state_dev_latch_time float           16422 
variable        DLT_starting_point        float           16604 
command         write_flow_characterization                 16520 
variable        test_data_read_control    unsigned        16628 
variable        steady_state_dev_alimit   float           16421 
command         write_device_test_status                  16590 
command         write_stiction_high_wlimit                 16565 
command         write_supply_pressure_latch_time                 16579 
command         read_histogram_data                       16715 
variable        valve_test_number         enumerated      16618 
command         write_cut_off_type                        16717 
command         write_supply_pressure_low_alimit                 16577 
variable        HART_error_rate_Value     float           16790 
method          set_quick_1_33_curve_method                 16446 
variable        spool_position_Value      float           16786 
variable        test_time_resolution      unsigned        16630 
item-array      event_times               variable        16699 
menu            warning_limits_menu                       16455 
variable        trend_data_10             float           16669 
variable        trend_data_11             float           16670 
variable        spool_reversals_wlimit    unsigned        16408 
variable        trend_data_12             float           16671 
variable        dev_temperature_low_alimit float           16418 
variable        trend_data_13             float           16672 
variable        trend_data_14             float           16673 
command         write_setpoint_cut_off_low                 16523 
variable        steady_state_dev_wlimit   float           16409 
variable        DLT_KF_testing_time       float           16488 
method          set_1_33_curve_method                     16445 
command         read_split_range_configuration                 16537 
variable        valve_reversals_wlimit    unsigned        16404 
variable        trend_data_0              float           16659 
variable        trend_data_1              float           16660 
variable        trend_data_2              float           16661 
variable        trend_data_3              float           16662 
variable        trend_data_4              float           16663 
variable        trend_data_5              float           16664 
command         write_valve_package_info                  16551 
variable        trend_data_6              float           16665 
variable        trend_data_7              float           16666 
variable        characterization_type     enumerated      16400 
variable        trend_data_8              float           16667 
variable        trend_data_9              float           16668 
command         read_characterization_table                 16745 
command         read_valve_characterization                 16517 
variable        event_time_10             float           16687 
command         write_travel_limits                       16525 
variable        control_value_Value       float           16772 
unit            pressure_units_2_relation                 16755 
command         read_valve_rotation_direction                 16747 
variable        MPST_KF_testing_time      float           16481 
method          start_vdt_method                          16474 
variable        bypass_signal_modifications enumerated      16390 
variable        VOAT_init_time            float           16616 
command         write_travel_rate_dec                     16528 
variable        no_of_events              unsigned        16676 
variable        use_limits                enumerated      16546 
variable        spool_valve_reversals_cntr float           16513 
variable        cylinder_pressure_C1_Value float           16776 
command         write_performance_level                   16532 
command         write_actuator_type                       16536 
menu            alarm_limits_menu                         16456 
menu            counters_menu                             16457 
item-array      event_numbers             variable        16698 
command         write_load_for_open_high_alimit                 16575 
collection      dv5_supply_pressure       variable        16766 
variable        temperature_Value         float           16784 
method          show_device_mode_method                   16463 
variable        DLT_KF_starting_point     float           16486 
collection      dv10_valve_setpoint       variable        16771 
variable        test_data_selector        unsigned        16627 
variable        valve_rotation_direction  enumerated      16386 
method          set_1_25_curve_method                     16443 
command         read_device_sno                           16593 
variable        DLT_KF_ending_point       float           16487 
variable        characterization_table_code unsigned        16516 
command         calib_loop_current                        16597 
variable        MPST_KF_gain              float           16485 
command         read_process_application_info                 16553 
collection      dv0_control_value         variable        16761 
variable        histogram_data_10         float           16713 
variable        histogram_data_11         float           16714 
variable        cal_current_select        unsigned        16596 
method          start_mpst_method                         16471 
method          device_lock_status                        16470 
command         write_valve_dead_angle                    16543 
command         write_actuator_package_info                 16541 
variable        test_data_last_index      unsigned        16629 
variable        VOAT_measurement_point    float           16613 
command         read_VC_board_sno                         16584 
variable        actuator_travel_cntr      float           16508 
method          set_linear_curve_method                   16442 
command         read_actuator_package_info                 16540 
variable        trend_data_item_selector  unsigned        16658 
menu            revision_numbers_menu                     16460 
variable        valve_reversals_cntr      float           16507 
variable        HART_board_sno            ascii           16466 
variable        DLT_ramp_time             float           16606 
command         write_valve_rotation_direction                 16748 
method          cancel_calibration_or_tuning                 16752 
menu            serial_numbers_menu                       16461 
variable        MPST_data_point_number    unsigned        16598 
command         read_actuator_type                        16535 
variable        MPST_step_time            float           16601 
variable        supply_pressure_high_alimit float           16416 
method          identify_nd9000_method                    16464 
method          set_1_50_curve_method                     16447 
variable        event_number_1            enumerated      16688 
variable        event_number_2            enumerated      16689 
variable        pressure_difference_Value float           16780 
variable        event_number_3            enumerated      16690 
menu            test_key_figures_menu                     16454 
variable        event_number_4            enumerated      16691 
variable        event_number_5            enumerated      16692 
variable        event_number_6            enumerated      16693 
variable        valve_type                enumerated      16384 
variable        event_number_7            enumerated      16694 
menu            HART_related_menu                         16462 
variable        load_for_open_latch_number float           16428 
variable        event_number_8            enumerated      16695 
variable        event_number_9            enumerated      16696 
variable        VOAT_KF_ramp_time         float           16496 
unit            pressure_units_1_relation                 16754 
variable        MPST_KF_ending_point      float           16480 
variable        VDT_starting_point        float           16609 
variable        valve_position_Value      float           16774 
command         init_dynamic_loop_test                    16608 
collection      dv8_loop_current          variable        16769 
variable        spool_total_travel_wlimit float           16407 
method          edit_charac_table_method                  16449 
command         write_travel_rate_inc                     16527 
command         write_stiction_low_wlimit                 16564 
variable        split_range_high          float           16399 
variable        total_op_time_wlimit      float           16402 
command         start_test                                16621 
variable        dev_var_code              unsigned        16515 
variable        dev_temperature_latch_time float           16420 
variable        cut_off_low               float           16396 
variable        VOAT_steady_time          float           16614 
method          show_device_status_method                 16459 
variable        VOAT_KF_SR_O2C_close      float           16501 
menu            signal_modifications_menu                 16439 
command         write_total_op_time_wlimit                 16555 
variable        supply_pressure_Value     float           16782 
menu            units_menu                                16436 
command         read_travel_speed_limits                  16526 
variable        setpoint_travel_cntr      float           16510 
command         write_supply_pressure_high_alimit                 16578 
variable        control_value_Units       enumerated      16773 
command         write_split_range_configuration                 16538 
variable        test_data_index           unsigned        16626 
command         read_performance_level                    16531 
method          warn_about_updating                       16751 
variable        MPST_init_time            float           16602 
command         read_device_test_status                   16589 
command         read_counter_data                         16701 
command         read_use_limits                           16547 
variable        load_for_open_high_wlimit float           16414 
command         reset_diagnostics                         16592 
menu            device_info_menu                          16435 
menu            calibrations_menu                         16432 
variable        travel_rate_inc           float           16394 
variable        DAC_board_SW_rev          ascii           16469 
variable        MPST_starting_point       float           16599 
variable        characterization_polynom_factor float           16401 
method          tuning_method                             16451 
variable        spool_position_Units      enumerated      16787 
command         read_setpoint_and_target_position_limits                 16522 
command         read_diagnostics_alarm_limits                 16583 
command         read_DLT_key_figures                      16623 
command         activate_self_calibration                 16530 
variable        VOAT_KF_SR_C2O_open       float           16504 
menu            parameters_menu                           16431 
command         write_characterization_table                 16746 
command         write_bypass_signal_modifications                 16545 
variable        VOAT_ramp_time            float           16615 
command         write_valve_type                          16534 
variable        positioner_fail_action    enumerated      16387 
variable        setpoint_reversals_trend_wlimit unsigned        16797 
variable        press_diff_minimum_span   float           16894 
variable        vlv_sp_sensor_serial_number integer         16941 
variable        cyl_press_C1_sensor_serial_number integer         16873 
variable        cyl_press_C2_upper_sensor_limit float           16883 
command         read_diagnostics_limits_part2                 16820 
variable        parameter_value_integer   integer         16811 
command         write_load_for_close_latch_number                 16829 
variable        press_diff_sensor_serial_number integer         16891 
variable        HART_error_rate_Status    bit-enumerated  16931 
variable        cyl_press_C1_upper_sensor_limit float           16874 
command         write_alarms_disabled                     16839 
command         read_parameter                            16813 
variable        calibration_status        unsigned        16830 
menu            dynamic_variables_menu                    16805 
variable        valve_setpoint_Status     bit-enumerated  16940 
variable        vlv_pos_lower_sensor_limit float           16866 
variable        parameter_value_float     float           16812 
variable        spool_pos_minimum_span    float           16917 
method          all_calibrations_method                   16804 
command         write_load_for_close_low_alimit                 16827 
command         write_valve_travel_trend_wlimit                 16823 
variable        valve_position_classification enumerated      16860 
method          cancel_any_calibration                    16849 
variable        ctrl_val_damping_value    float           16859 
variable        loop_curr_sensor_serial_number integer         16923 
variable        valve_reversals_ssp_trend_wlimit unsigned        16796 
variable        load_for_close_low_wlimit float           16798 
variable        spool_position_PDQ        enumerated      16911 
variable        load_for_close_high_alimit float           16801 
command         read_selected_events_1                    16815 
command         read_selected_events_2                    16848 
variable        loop_curr_lower_sensor_limit float           16925 
variable        supply_pressure_damping_value float           16904 
variable        temp_sensor_serial_number integer         16909 
method          read_selected_events_method                 16808 
variable        pressure_difference_PDQ   enumerated      16888 
variable        valve_reversals_trend_wlimit unsigned        16795 
variable        loop_curr_damping_value   float           16927 
command         write_load_for_close_high_alimit                 16828 
command         start_calibration                         16837 
variable        HART_err_lower_sensor_limit float           16934 
variable        temperature_classification enumerated      16905 
variable        valve_setpoint_classification enumerated      16937 
command         write_setpoint_reversals_trend_wlimit                 16822 
variable        valve_position_PDQ        enumerated      16861 
command         cancel_calibration                        16834 
variable        test_start_code           unsigned        16840 
variable        pressure_difference_LS    enumerated      16889 
variable        loop_current_PDQ          enumerated      16920 
command         write_valve_reversals_trend_wlimit                 16821 
variable        control_value_PDQ         enumerated      16852 
variable        HART_err_damping_value    float           16936 
variable        pressure_difference_Status bit-enumerated  16890 
variable        ctrl_val_sensor_serial_number integer         16855 
variable        pressure_difference_classification enumerated      16887 
variable        calib_parameter           float           16836 
variable        valve_setpoint_LS         enumerated      16939 
variable        loop_current_classification enumerated      16919 
variable        vlv_sp_damping_value      float           16945 
variable        HART_err_sensor_serial_number integer         16932 
method          set_predefined_curve_method                 16806 
variable        spool_pos_upper_sensor_limit float           16915 
variable        supply_pressure_Status    bit-enumerated  16899 
variable        calib_request             unsigned        16835 
variable        test_status_code          unsigned        16844 
command         get_calibration_status                    16833 
variable        ctrl_val_upper_sensor_limit float           16856 
variable        spool_position_classification enumerated      16910 
variable        cylinder_pressure_C1_LS   enumerated      16871 
variable        press_diff_upper_sensor_limit float           16892 
variable        HART_error_rate_PDQ       enumerated      16929 
variable        control_value_LS          enumerated      16853 
variable        loop_current_Status       bit-enumerated  16922 
variable        calibration_sub_state     unsigned        16831 
command         write_valve_reversals_ssp_trend_wlimit                 16824 
variable        valve_setpoint_PDQ        enumerated      16938 
variable        spool_pos_lower_sensor_limit float           16916 
variable        current_turning_angle     float           16816 
variable        press_diff_damping_value  float           16895 
variable        cylinder_pressure_C2_LS   enumerated      16880 
variable        cyl_press_C1_damping_value float           16877 
variable        supply_pressure_minimum_span float           16903 
variable        valve_position_LS         enumerated      16862 
variable        spool_pos_sensor_serial_number integer         16914 
variable        cylinder_pressure_C2_classification enumerated      16878 
method          modify_parameters_method                  16850 
variable        cylinder_pressure_C1_classification enumerated      16869 
variable        load_for_close_latch_number float           16802 
variable        vlv_sp_lower_sensor_limit float           16943 
variable        spool_pos_damping_value   float           16918 
variable        parameter_number          unsigned        16809 
variable        supply_pressure_LS        enumerated      16898 
command         write_new_turning_angle                   16819 
command         write_load_for_close_low_wlimit                 16825 
variable        valve_travel_trend_wlimit float           16794 
variable        parameter_type            enumerated      16810 
variable        cylinder_pressure_C2_PDQ  enumerated      16879 
variable        vlv_sp_upper_sensor_limit float           16942 
variable        new_turning_angle         float           16818 
variable        calibration_error_code    unsigned        16832 
command         general_get_test_status                   16846 
variable        cylinder_pressure_C1_Status bit-enumerated  16872 
variable        ctrl_val_minimum_span     float           16858 
variable        cylinder_pressure_C2_Status bit-enumerated  16881 
variable        HART_err_upper_sensor_limit float           16933 
command         start_event_read                          16847 
variable        spool_position_LS         enumerated      16912 
variable        HART_error_rate_classification enumerated      16928 
variable        cylinder_pressure_C1_PDQ  enumerated      16870 
variable        supply_pressure_PDQ       enumerated      16897 
variable        alarms_disabled           enumerated      16803 
command         general_start_test                        16842 
variable        load_for_close_high_wlimit float           16799 
variable        loop_curr_minimum_span    float           16926 
variable        control_value_classification enumerated      16851 
variable        temperature_PDQ           enumerated      16906 
variable        cyl_press_C2_minimum_span float           16885 
variable        cyl_press_C2_damping_value float           16886 
variable        cyl_press_C1_minimum_span float           16876 
variable        vlv_sp_minimum_span       float           16944 
command         write_parameter                           16814 
variable        valve_position_Status     bit-enumerated  16863 
variable        supply_pressure_classification enumerated      16896 
command         general_cancel_test                       16843 
method          start_offline_tests_method                 16807 
variable        vlv_pos_minimum_span      float           16867 
variable        HART_err_minimum_span     float           16935 
variable        temperature_LS            enumerated      16907 
variable        temperature_Status        bit-enumerated  16908 
variable        cyl_press_C2_sensor_serial_number integer         16882 
variable        supply_pressure_sensor_serial_number integer         16900 
variable        vlv_pos_upper_sensor_limit float           16865 
variable        vlv_pos_sensor_serial_number integer         16864 
command         write_load_for_close_high_wlimit                 16826 
variable        test_error_code           unsigned        16845 
variable        cyl_press_C2_lower_sensor_limit float           16884 
variable        loop_current_LS           enumerated      16921 
variable        ctrl_val_lower_sensor_limit float           16857 
variable        cyl_press_C1_lower_sensor_limit float           16875 
variable        vlv_pos_damping_value     float           16868 
variable        points_in_mpst            unsigned        16841 
variable        control_value_Status      bit-enumerated  16854 
command         read_alarms_disabled                      16838 
variable        press_diff_lower_sensor_limit float           16893 
variable        load_for_close_low_alimit float           16800 
variable        HART_error_rate_LS        enumerated      16930 
command         read_current_turning_angle                 16817 
variable        supply_pressure_lower_sensor_limit float           16902 
variable        supply_pressure_upper_sensor_limit float           16901 
variable        loop_curr_upper_sensor_limit float           16924 
variable        spool_position_Status     bit-enumerated  16913 
